## Zend_Measure_Current

Description

- license: New BSD License
- copyright: Copyright (c) 2005-2007 Zend Technologies USA Inc. (http://www.zend.com)

Located in /Zend/Measure/Current.php (line 38)

    Zend_Measure_Abstract
       |
       --Zend_Measure_Current

Class Constant Summary
ABAMPERE = 'ABAMPERE'
AMPERE = 'AMPERE'
BIOT = 'BIOT'
CENTIAMPERE = 'CENTIAMPERE'
COULOMB_PER_SECOND = 'COULOMB_PER_SECOND'
DECIAMPERE = 'DECIAMPERE'
DEKAAMPERE = 'DEKAAMPERE'
ELECTROMAGNETIC_UNIT = 'ELECTROMAGNATIC_UNIT'
ELECTROSTATIC_UNIT = 'ELECTROSTATIC_UNIT'
FRANCLIN_PER_SECOND = 'FRANCLIN_PER_SECOND'
GAUSSIAN = 'GAUSSIAN'
GIGAAMPERE = 'GIGAAMPERE'
GILBERT = 'GILBERT'
HECTOAMPERE = 'HECTOAMPERE'
KILOAMPERE = 'KILOAMPERE'
MEGAAMPERE = 'MEGAAMPERE'
MICROAMPERE = 'MICROAMPERE'
MILLIAMPERE = 'MILLIAMPERE'
NANOAMPERE = 'NANOAMPERE'
PICOAMPERE = 'PICOAMPERE'
SIEMENS_VOLT = 'SIEMENS_VOLT'
STANDARD = 'AMPERE'
STATAMPERE = 'STATAMPERE'
TERAAMPERE = 'TERAAMPERE'
VOLT_PER_OHM = 'VOLT_PER_OHM'
WATT_PER_VOLT = 'WATT_PER_VOLT'
WEBER_PER_HENRY = 'WEBER_PER_HENRY'
Variable Summary
mixed $_UNITS
Variables
mixed $_UNITS = array(
'ABAMPERE' => array(10, 'abampere'),'AMPERE'=>array(1,'A'),'BIOT'=>array(10,'Bi'),'CENTIAMPERE'=>array(0.01,'cA'),'COULOMB_PER_SECOND'=>array(1,'C/s'),'DECIAMPERE'=>array(0.1,'dA'),'DEKAAMPERE'=>array(10,'daA'),'ELECTROMAGNATIC_UNIT'=>array(10,'current emu'),'ELECTROSTATIC_UNIT'=>array(3.335641e-10,'current esu'),'FRANCLIN_PER_SECOND'=>array(3.335641e-10,'Fr/s'),'GAUSSIAN'=>array(3.335641e-10,'G current'),'GIGAAMPERE'=>array(1.0e+9,'GA'),'GILBERT'=>array(0.79577472,'Gi'),'HECTOAMPERE'=>array(100,'hA'),'KILOAMPERE'=>array(1000,'kA'),'MEGAAMPERE'=>array(1000000,'MA'),'MICROAMPERE'=>array(0.000001,'µA'),'MILLIAMPERE'=>array(0.001,'mA'),'NANOAMPERE'=>array(1.0e-9,'nA'),'PICOAMPERE'=>array(1.0e-12,'pA'),'SIEMENS_VOLT'=>array(1,'SV'),'STATAMPERE'=>array(3.335641e-10,'statampere'),'TERAAMPERE'=>array(1.0e+12,'TA'),'VOLT_PER_OHM'=>array(1,'V/Ohm'),'WATT_PER_VOLT'=>array(1,'W/V'),'WEBER_PER_HENRY'=>array(1,'Wb/H'),'STANDARD'=>'AMPERE') (line 70)

- access: protected

Redefinition of:

Zend_Measure_Abstract::$_UNITS
  Unit types for this measurement

#### Inherited Variables

Inherited from Zend_Measure_Abstract

> Zend_Measure_Abstract::$_Locale
> Zend_Measure_Abstract::$_type
> Zend_Measure_Abstract::$_value

Methods

#### Inherited Methods

Inherited From Zend_Measure_Abstract

> Zend_Measure_Abstract::__construct()
> Zend_Measure_Abstract::add()
> Zend_Measure_Abstract::compare()
> Zend_Measure_Abstract::convertTo()
> Zend_Measure_Abstract::equals()
> Zend_Measure_Abstract::getConversionList()
> Zend_Measure_Abstract::getType()
> Zend_Measure_Abstract::getValue()
> Zend_Measure_Abstract::setType()
> Zend_Measure_Abstract::setValue()
> Zend_Measure_Abstract::sub()
> Zend_Measure_Abstract::toString()
> Zend_Measure_Abstract::__toString()

Class Constants
ABAMPERE = 'ABAMPERE' (line 43)
AMPERE = 'AMPERE' (line 44)
BIOT = 'BIOT' (line 45)
CENTIAMPERE = 'CENTIAMPERE' (line 46)
COULOMB_PER_SECOND = 'COULOMB_PER_SECOND' (line 47)
DECIAMPERE = 'DECIAMPERE' (line 48)
DEKAAMPERE = 'DEKAAMPERE' (line 49)
ELECTROMAGNETIC_UNIT = 'ELECTROMAGNATIC_UNIT' (line 50)
ELECTROSTATIC_UNIT = 'ELECTROSTATIC_UNIT' (line 51)
FRANCLIN_PER_SECOND = 'FRANCLIN_PER_SECOND' (line 52)
GAUSSIAN = 'GAUSSIAN' (line 53)
GIGAAMPERE = 'GIGAAMPERE' (line 54)
GILBERT = 'GILBERT' (line 55)
HECTOAMPERE = 'HECTOAMPERE' (line 56)
KILOAMPERE = 'KILOAMPERE' (line 57)
MEGAAMPERE = 'MEGAAMPERE' (line 58)
MICROAMPERE = 'MICROAMPERE' (line 59)
MILLIAMPERE = 'MILLIAMPERE' (line 60)
NANOAMPERE = 'NANOAMPERE' (line 61)
PICOAMPERE = 'PICOAMPERE' (line 62)
SIEMENS_VOLT = 'SIEMENS_VOLT' (line 63)
STANDARD = 'AMPERE' (line 41)
STATAMPERE = 'STATAMPERE' (line 64)
TERAAMPERE = 'TERAAMPERE' (line 65)
VOLT_PER_OHM = 'VOLT_PER_OHM' (line 66)
WATT_PER_VOLT = 'WATT_PER_VOLT' (line 67)
WEBER_PER_HENRY = 'WEBER_PER_HENRY' (line 68)

Documentation generated on Wed, 21 Feb 2007 11:46:31 -0800 by phpDocumentor 1.3.1